(2017-03-20 15:08:53):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-03-20 15:08:53):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-03-20 15:08:54):Succeed in initializing IS_OPERA.

(2017-03-20 17:48:44):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-03-20 17:48:44):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-03-20 17:48:45):Succeed in initializing IS_OPERA.

(2017-03-20 17:48:54):Set the local Database to : IS620P_V10.0.mdb

(2017-03-20 17:48:56):Set the local Database to : IS620P_V10.0_E.mdb

(2017-03-20 18:00:47):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-03-20 18:00:47):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-03-20 18:00:48):Succeed in initializing IS_OPERA.

(2017-03-20 18:05:44):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-03-20 18:05:44):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-03-20 18:05:45):Succeed in initializing IS_OPERA.

(2017-03-21 15:35:22):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-03-21 15:35:22):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-03-21 15:35:23):Succeed in initializing IS_OPERA.

(2017-03-21 16:05:35):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-03-21 16:05:35):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-03-21 16:05:36):Succeed in initializing IS_OPERA.

(2017-03-21 16:41:39):Software reset succeeds.

(2017-03-28 19:01:27):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-03-28 19:01:27):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-03-28 19:01:28):Succeed in initializing IS_OPERA.

(2017-04-07 18:14:01):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-04-07 18:14:01):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-04-07 18:14:02):Succeed in initializing IS_OPERA.

(2017-06-01 10:41:34):No serial port available, check serial hardware.

(2017-06-01 10:41:35):Succeed in initializing IS_OPERA.

(2017-06-01 12:30:38):Find a servo connection: 1. Serial port No.: COM11
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-01 12:30:38):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-06-01 12:30:39):Succeed in initializing IS_OPERA.

(2017-06-01 12:34:54):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-01 12:34:54):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-06-01 12:34:55):Succeed in initializing IS_OPERA.

(2017-06-01 12:35:12):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-01 12:35:12):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-06-01 12:35:13):Succeed in initializing IS_OPERA.

(2017-06-01 12:36:13):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-01 12:36:13):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-06-01 12:36:14):Succeed in initializing IS_OPERA.

(2017-06-01 12:36:56):[data exceeding range]:[function code H0517][range 35-32767][running value 0]

(2017-06-01 12:36:56):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-01 12:36:56):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-01 12:36:56):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-01 12:36:56):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-01 12:36:56):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-01 12:36:56):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-01 14:35:39):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-01 14:35:39):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-06-01 14:35:40):Succeed in initializing IS_OPERA.

(2017-06-01 14:37:21):[data exceeding range]:[function code H0517][range 35-32767][running value 0]

(2017-06-01 14:37:21):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-01 14:37:21):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-01 14:37:21):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-01 14:37:21):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-01 14:37:21):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-01 14:37:21):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-01 14:41:09):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-01 14:41:09):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-01 14:41:09):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-01 14:41:09):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-01 14:41:09):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-01 14:41:09):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-01 14:51:33):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-01 14:51:33):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-01 15:27:27):[data exceeding range]:[function code H0517][range 35-32767][running value 0]

(2017-06-01 15:27:27):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-01 15:27:27):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-01 16:40:03):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-01 16:40:03):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-01 18:10:58):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-01 18:10:58):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-06-01 18:10:59):Succeed in initializing IS_OPERA.

(2017-06-01 18:24:51):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-01 18:24:51):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-01 18:24:51):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-01 18:24:51):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-01 18:24:51):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-01 18:24:51):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-02 10:55:27):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-02 10:55:27):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-06-02 10:55:28):Succeed in initializing IS_OPERA.

(2017-06-02 11:05:24):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-02 11:05:24):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-02 11:28:27):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-02 11:28:27):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-02 11:28:27):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-02 11:28:27):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-02 14:37:56):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-02 14:37:56):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-02 14:37:56):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-02 14:37:56):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-02 15:30:26):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-02 15:30:26):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-02 15:30:26):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-02 15:30:26):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-02 15:31:13):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-02 15:31:13):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-02 15:31:13):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-02 15:31:13):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-02 15:36:46):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-02 15:36:46):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-02 15:36:46):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-02 15:36:46):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-02 15:54:51):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-02 15:54:51):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-06-02 15:54:52):Succeed in initializing IS_OPERA.

(2017-06-02 16:23:22):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-02 16:23:22):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-02 16:23:22):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-02 16:23:22):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-02 16:23:38):[data exceeding range]:[function code H0517][range 35-32767][running value 0]

(2017-06-02 16:23:38):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-02 16:23:38):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-02 16:59:05):No serial port available, check serial hardware.

(2017-06-02 16:59:07):Succeed in initializing IS_OPERA.

(2017-06-02 17:02:42):Set the local Database to : IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-02 17:12:26):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-02 17:12:26):Current software version of the servo:  00000001, database: IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-02 17:12:27):Succeed in initializing IS_OPERA.

(2017-06-02 17:13:27):[data exceeding range]:[function code H0517][range 35-32767][running value 0]

(2017-06-02 17:13:27):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-02 17:13:27):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-02 17:13:27):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-02 17:13:27):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-02 17:13:27):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-02 17:13:27):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-28 11:11:33):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-28 11:11:33):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-06-28 11:11:34):Succeed in initializing IS_OPERA.

(2017-06-28 11:14:17):Set the local Database to : IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 11:19:29):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-28 11:19:29):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-28 11:19:29):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-28 11:19:29):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-28 11:19:29):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-28 11:19:29):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-28 11:19:29):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65533]

(2017-06-28 11:19:29):[data exceeding range]:[function code H0B22][range -1200-1200][running value 65532]

(2017-06-28 11:33:30):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-28 11:33:30):Current software version of the servo:  00000001, database: IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 11:33:31):Succeed in initializing IS_OPERA.

(2017-06-28 11:33:46):Set the local Database to : IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 11:37:39):Software reset succeeds.

(2017-06-28 11:41:34):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-28 11:41:34):Current software version of the servo:  00000001, database: IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 11:53:01):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-28 11:53:01):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-28 11:53:01):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-28 11:53:01):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-28 11:53:01):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-28 11:53:01):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-28 11:53:01):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65533]

(2017-06-28 11:53:01):[data exceeding range]:[function code H0B22][range -1200-1200][running value 65532]

(2017-06-28 13:24:03):Serial port 7 is not connected to the device.

(2017-06-28 13:24:11):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-28 13:24:11):Current software version of the servo:  00000001, database: IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 13:26:26):Software reset fails
Error code: 00000004.

(2017-06-28 13:26:56):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-28 13:26:56):Current software version of the servo:  00000001, database: IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 14:01:28):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-28 14:01:28):Current software version of the servo:  00000001, database: IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 14:17:40):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-28 14:17:40):Current software version of the servo:  00000001, database: IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 14:27:41):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-28 14:27:41):Current software version of the servo:  00000001, database: IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 14:45:45):Find a servo connection: 1. Serial port No.: COM7
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-06-28 14:45:45):Current software version of the servo:  00000001, database: IS620P&IS600P_DDRV1.0_E.mdb

(2017-06-28 14:46:34):[data exceeding range]:[function code H0517][range 35-32767][running value 0]

(2017-06-28 14:46:34):[data exceeding range]:[function code H0550][range 1-65535][running value 0]

(2017-06-28 14:46:34):[data exceeding range]:[function code H0551][range 1-65535][running value 0]

(2017-06-28 14:46:34):[data exceeding range]:[function code H0709][range 0-3000][running value 3500]

(2017-06-28 14:46:34):[data exceeding range]:[function code H0710][range 0-3000][running value 3500]

(2017-06-28 14:46:34):[data exceeding range]:[function code H0711][range 0-3000][running value 3500]

(2017-06-28 14:46:34):[data exceeding range]:[function code H0712][range 0-3000][running value 3500]

(2017-06-28 14:46:34):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65533]

(2017-06-28 14:46:34):[data exceeding range]:[function code H0B22][range -1200-1200][running value 65533]

(2017-06-28 17:26:35):No serial port available, check serial hardware.

(2017-06-28 17:26:41):Succeed in initializing IS_OPERA.

(2017-06-29 09:36:20):No serial port available, check serial hardware.

(2017-06-29 09:36:22):Succeed in initializing IS_OPERA.

(2017-06-29 11:56:31):No serial port available, check serial hardware.

(2017-06-29 11:56:32):Succeed in initializing IS_OPERA.

(2017-07-05 11:08:49):No serial port available, check serial hardware.

(2017-07-05 11:08:51):Succeed in initializing IS_OPERA.

(2017-07-06 07:20:29):No serial port available, check serial hardware.

(2017-07-06 07:20:31):Succeed in initializing IS_OPERA.

(2017-07-06 07:41:35):No serial port available, check serial hardware.

(2017-07-06 07:41:37):Succeed in initializing IS_OPERA.

(2017-07-06 07:42:16):Set the local Database to : IS620P_V10.0_E.mdb

(2017-07-06 07:42:43):No serial port available, check serial hardware.

(2017-07-06 07:42:45):Succeed in initializing IS_OPERA.

(2017-07-06 09:29:37):No serial port available, check serial hardware.

(2017-07-06 09:29:39):Succeed in initializing IS_OPERA.

(2017-07-06 13:24:52):No serial port available, check serial hardware.

(2017-07-06 13:24:54):Succeed in initializing IS_OPERA.

(2017-08-09 19:47:36):Find a servo connection: 1. Serial port No.: COM1
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-08-09 19:47:36):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-08-09 19:47:38):Succeed in initializing IS_OPERA.

(2017-08-09 19:49:12):Save a recipe file: C:\Users\T07\Desktop\20170809194904[IS620P_V].txt

(2017-08-09 19:54:51):Find a servo connection: 1. Serial port No.: COM1
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-08-09 19:54:51):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-08-09 19:54:52):Succeed in initializing IS_OPERA.

(2017-08-18 17:46:51):No serial port available, check serial hardware.

(2017-08-18 17:46:53):Succeed in initializing IS_OPERA.

(2017-09-01 15:59:36):Find a servo connection: 1. Serial port No.: COM1
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-09-01 15:59:36):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-09-01 15:59:37):Succeed in initializing IS_OPERA.

(2017-09-04 10:47:02):No serial port available, check serial hardware.

(2017-09-04 10:47:05):Succeed in initializing IS_OPERA.

(2017-09-07 07:35:45):No serial port available, check serial hardware.

(2017-09-07 07:35:47):Succeed in initializing IS_OPERA.

(2017-09-12 09:15:36):No serial port available, check serial hardware.

(2017-09-12 09:15:43):Succeed in initializing IS_OPERA.

(2017-09-13 09:55:26):No serial port available, check serial hardware.

(2017-09-13 09:55:28):Succeed in initializing IS_OPERA.

(2017-09-13 11:11:54):Serial port 2 is not connected to the device.

(2017-09-13 11:11:54):Completing search. No device is connected or serial port is used.

(2017-09-13 11:11:55):Succeed in initializing IS_OPERA.

(2017-09-13 11:12:11):8-N-2Fail to connect device.

(2017-09-13 11:12:17):8-N-2Fail to connect device.

(2017-09-13 11:13:48):8-N-2Fail to connect device.

(2017-09-13 11:14:01):8-E-1Fail to connect device.

(2017-09-13 11:14:07):8-O-1Fail to connect device.

(2017-09-13 11:14:13):8-N-1Fail to connect device.

(2017-09-13 11:14:19):8-N-2Fail to connect device.

(2017-09-13 11:14:28):8-N-2Fail to connect device.

(2017-09-13 11:14:35):8-N-2Fail to connect device.

(2017-09-13 11:14:41):8-N-2Fail to connect device.

(2017-09-13 11:14:48):8-N-2Fail to connect device.

(2017-09-13 11:14:54):8-N-2Fail to connect device.

(2017-09-13 11:16:40):8-N-2Fail to connect device.

(2017-09-13 11:16:45):8-N-2Device connected successfully.

(2017-09-13 11:30:02):[data exceeding range]:[function code H0012][range 10-65535][running value 0]

(2017-09-13 11:30:02):[data exceeding range]:[function code H0019][range 1-65535][running value 0]

(2017-09-13 11:30:02):[data exceeding range]:[function code H0020][range 1-65535][running value 0]

(2017-09-13 11:30:02):[data exceeding range]:[function code H0021][range 1-65535][running value 0]

(2017-09-13 11:30:40):[data exceeding range]:[function code H0233][range 0-0][running value 2000]

(2017-09-13 11:30:40):[data exceeding range]:[function code H0B58][range 0-65535][running value -1]

(2017-09-13 11:30:40):[data exceeding range]:[function code H0B71][range 0-65535][running value 7701704]

(2017-09-13 11:30:40):[data exceeding range]:[function code H0C14][range 1-4][running value 0]

(2017-09-13 11:30:40):[data exceeding range]:[function code H0F13][range 10-65535][running value 0]

(2017-09-13 11:31:43):Save a recipe file: E:\Projects\Kushal Automation\400W_20170913113049[IS620N_V].txt

(2017-09-13 11:32:01):No serial port available, check serial hardware.

(2017-09-13 11:32:03):Succeed in initializing IS_OPERA.

(2017-09-13 11:32:08):Read a recipe file: E:\Projects\Kushal Automation\400W_20170913113049[IS620N_V].txtInfo.:IS620N_V1.0_E.mdb


(2017-09-13 11:32:08):[exceeding range]:[function code H0233][range 0-0][current value 2000]

(2017-09-13 11:32:10):[exceeding range]:[function code H0B58][range 0-65535][current value -1]

(2017-09-13 11:32:11):[exceeding range]:[function code H0B71][range 0-65535][current value 7701704]

(2017-09-13 11:32:11):[exceeding range]:[function code H0C14][range 1-4][current value 0]

(2017-09-13 11:32:12):[exceeding range]:[function code H0F13][range 10-65535][current value 0]

(2017-09-13 11:32:23):8-N-2Device connected successfully.

(2017-09-13 12:00:42):8-N-2Device connected successfully.

(2017-09-13 12:00:53):[exceeding range]:[function code H0233][range 0-0][current value 2000]

(2017-09-13 12:00:54):[exceeding range]:[function code H0B58][range 0-65535][current value -1]

(2017-09-13 12:00:55):[exceeding range]:[function code H0B71][range 0-65535][current value 7701704]

(2017-09-13 12:00:56):[exceeding range]:[function code H0C14][range 1-4][current value 0]

(2017-09-13 12:00:56):[exceeding range]:[function code H0F13][range 10-65535][current value 0]

(2017-09-13 12:01:31):[data exceeding range]:[function code H0012][range 10-65535][running value 0]

(2017-09-13 12:01:31):[data exceeding range]:[function code H0017][range 2-360][running value 0]

(2017-09-13 12:02:12):[data exceeding range]:[function code H0233][range 0-0][running value 2000]

(2017-09-13 12:02:12):[data exceeding range]:[function code H0B58][range 0-65535][running value -8356153]

(2017-09-13 12:02:12):[data exceeding range]:[function code H0B60][range 0-65535][running value -1]

(2017-09-13 12:02:12):[data exceeding range]:[function code H0B71][range 0-65535][running value 7734159]

(2017-09-13 12:02:12):[data exceeding range]:[function code H0C04][range 0-0][running value 2]

(2017-09-13 12:02:12):[data exceeding range]:[function code H0F13][range 10-65535][running value 0]

(2017-09-13 17:00:07):Read a recipe file: E:\Projects\Kushal Automation\400W_20170913113049[IS620N_V].txtInfo.:IS620N_V1.0_E.mdb


(2017-09-13 17:00:07):[exceeding range]:[function code H0233][range 0-0][current value 2000]

(2017-09-13 17:00:08):[exceeding range]:[function code H0B58][range 0-65535][current value -1]

(2017-09-13 17:00:09):[exceeding range]:[function code H0B71][range 0-65535][current value 7701704]

(2017-09-13 17:00:09):[exceeding range]:[function code H0C14][range 1-4][current value 0]

(2017-09-13 17:00:10):[exceeding range]:[function code H0F13][range 10-65535][current value 0]

(2017-09-13 17:00:25):[exceeding range]:[function code H0233][range 0-0][current value 2000]

(2017-09-13 17:00:27):[exceeding range]:[function code H0B58][range 0-65535][current value -1]

(2017-09-13 17:00:28):[exceeding range]:[function code H0B71][range 0-65535][current value 7701704]

(2017-09-13 17:00:28):[exceeding range]:[function code H0C14][range 1-4][current value 0]

(2017-09-13 17:00:28):[exceeding range]:[function code H0F13][range 10-65535][current value 0]

(2017-09-13 17:00:37):Read a recipe file: E:\Projects\Kushal Automation\400W_20170913113049[IS620N_V].txtInfo.:IS620N_V1.0_E.mdb


(2017-09-13 17:00:37):[exceeding range]:[function code H0233][range 0-0][current value 2000]

(2017-09-13 17:00:39):[exceeding range]:[function code H0B58][range 0-65535][current value -1]

(2017-09-13 17:00:39):[exceeding range]:[function code H0B71][range 0-65535][current value 7701704]

(2017-09-13 17:00:39):[exceeding range]:[function code H0C14][range 1-4][current value 0]

(2017-09-13 17:00:40):[exceeding range]:[function code H0F13][range 10-65535][current value 0]

(2017-09-13 17:07:45):8-N-2Device connected successfully.

(2017-09-13 17:10:29):Save a recipe file: E:\Projects\Kushal Automation\400W_20170913113049[IS620N_V].txt

(2017-09-13 17:11:19):[data exceeding range]:[function code H0022][range 1-65535][running value 0]

(2017-09-13 17:14:10):[data exceeding range]:[function code H0022][range 1-65535][running value 0]

(2017-09-13 17:15:08):Save a recipe file: E:\Projects\Kushal Automation\750W_20170913171457[IS620N_V].txt

(2017-09-18 11:28:49):No serial port available, check serial hardware.

(2017-09-18 11:28:52):Succeed in initializing IS_OPERA.

(2017-09-21 16:28:02):No serial port available, check serial hardware.

(2017-09-21 16:28:04):Succeed in initializing IS_OPERA.

(2017-09-21 17:17:03):No serial port available, check serial hardware.

(2017-09-21 17:17:05):Succeed in initializing IS_OPERA.

(2017-09-26 15:28:51):No serial port available, check serial hardware.

(2017-09-26 15:28:54):Succeed in initializing IS_OPERA.

(2017-09-29 12:13:26):No serial port available, check serial hardware.

(2017-09-29 12:13:28):Succeed in initializing IS_OPERA.

(2017-09-29 12:28:36):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-09-29 12:28:36):Current software version of the servo:  00000001, database: IS620N_V1.0_E.mdb

(2017-09-29 12:28:36):Succeed in initializing IS_OPERA.

(2017-09-29 12:29:08):[data exceeding range]:[function code H0233][range 0-0][running value 2000]

(2017-09-29 12:29:08):[data exceeding range]:[function code H0B58][range 0-65535][running value -10]

(2017-09-29 12:29:08):[data exceeding range]:[function code H0B60][range 0-65535][running value -1]

(2017-09-29 12:29:08):[data exceeding range]:[function code H0B71][range 0-65535][running value 1023974]

(2017-09-29 12:29:08):[data exceeding range]:[function code H0C04][range 0-0][running value 1001]

(2017-09-29 12:29:08):[data exceeding range]:[function code H0C14][range 1-4][running value 0]

(2017-09-29 12:29:08):[data exceeding range]:[function code H0F13][range 10-65535][running value 0]

(2017-09-29 12:29:51):[data exceeding range]:[function code H0011][range 1-65535][running value 0]

(2017-09-29 12:29:51):[data exceeding range]:[function code H0023][range 1-65535][running value 0]

(2017-09-29 12:32:50):[data exceeding range]:[function code H0014][range 100-9000][running value 0]

(2017-09-29 12:32:50):[data exceeding range]:[function code H0031][range 1-1073741824][running value 0]

(2017-09-29 15:01:14):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-09-29 15:01:14):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-09-29 15:01:15):Succeed in initializing IS_OPERA.

(2017-10-05 13:06:26):No serial port available, check serial hardware.

(2017-10-05 13:06:28):Succeed in initializing IS_OPERA.

(2017-10-05 13:08:14):No serial port available, check serial hardware.

(2017-10-05 13:08:16):Succeed in initializing IS_OPERA.

(2017-10-05 13:09:06):Read a recipe file: E:\Projects\Riddhi Diamond\RIDDHI_DIAMOND\Y_Axis\Upload_20171004094452[IS620P_V].txtInfo.:IS620P_V10.0_E.mdb


(2017-10-05 13:09:06):[exceeding range]:[function code H0105][range 1-65535][current value 0]

(2017-10-05 13:09:07):[exceeding range]:[function code H0124][range 1-65535][current value 0]

(2017-10-05 13:33:00):No serial port available, check serial hardware.

(2017-10-05 13:33:02):Succeed in initializing IS_OPERA.

(2017-10-05 14:01:05):No serial port available, check serial hardware.

(2017-10-05 14:01:07):Succeed in initializing IS_OPERA.

(2017-10-05 14:26:26):No serial port available, check serial hardware.

(2017-10-05 14:26:28):Succeed in initializing IS_OPERA.

(2017-10-05 17:20:11):8-N-2Device connected successfully.

(2017-10-05 17:30:32):Read a recipe file: C:\Users\T07\Desktop\IS620P_CO_multiposition_05_10_17[IS620P_V].txtInfo.:IS620P_V10.0_E.mdb


(2017-10-05 17:30:34):[exceeding range]:[function code H0200][range 0-6][current value 8]

(2017-10-05 17:30:36):[exceeding range]:[function code H0B21][range -1200-1200][current value 65535]

(2017-10-05 17:31:45):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65534]

(2017-10-05 17:39:42):Set the local Database to : IS620P_V10.0_E.mdb

(2017-10-05 17:40:45):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65535]

(2017-10-05 17:43:10):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65534]

(2017-10-05 17:43:30):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65534]

(2017-10-05 18:17:07):Read a recipe file: C:\Users\T07\Desktop\IS620P_CO_multiposition_05_10_17[IS620P_V].txtInfo.:IS620P_V10.0_E.mdb


(2017-10-05 18:17:07):[exceeding range]:[function code H0200][range 0-6][current value 8]

(2017-10-05 18:17:08):[exceeding range]:[function code H0B21][range -1200-1200][current value 65535]

(2017-10-05 20:09:56):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-10-05 20:09:56):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-10-05 20:09:57):Succeed in initializing IS_OPERA.

(2017-10-05 20:12:09):Save a recipe file: C:\Users\T07\Desktop\IS620P_Multi-position_20171005201144[IS620P_V].txt

(2017-10-05 20:15:26):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-10-05 20:15:26):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-10-05 20:15:26):Succeed in initializing IS_OPERA.

(2017-10-06 13:36:52):No serial port available, check serial hardware.

(2017-10-06 13:36:55):Succeed in initializing IS_OPERA.

(2017-10-24 16:07:02):No serial port available, check serial hardware.

(2017-10-24 16:07:06):Succeed in initializing IS_OPERA.

(2017-10-24 16:11:08):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-10-24 16:11:08):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-10-24 16:24:26):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2017-10-24 16:24:26):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2017-10-24 16:24:27):Succeed in initializing IS_OPERA.

(2017-10-24 16:24:48):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65534]

(2017-10-24 16:36:14):Serial port 2 is not connected to the device.

(2017-10-24 16:36:15):Succeed in initializing IS_OPERA.

(2017-10-24 16:49:50):Completing search. No device is connected or serial port is used.

(2017-10-24 16:49:50):Succeed in initializing IS_OPERA.

(2017-10-24 16:50:01):COM2 serial port is being used.

(2017-10-24 16:50:09):8-N-2Device connected successfully.

(2017-10-24 16:50:41):[data exceeding range]:[function code H0B71][range 0-65535][running value 1042970]

(2017-10-24 16:50:41):[data exceeding range]:[function code H0C35][range 4-20][running value 0]

(2017-10-24 16:50:41):[data exceeding range]:[function code H0F13][range 10-65535][running value 0]

(2017-10-24 17:38:44):No serial port available, check serial hardware.

(2017-10-24 17:38:46):Succeed in initializing IS_OPERA.

(2017-10-30 14:49:26):No serial port available, check serial hardware.

(2017-10-30 14:49:29):Succeed in initializing IS_OPERA.

(2017-10-31 16:05:57):No serial port available, check serial hardware.

(2017-10-31 16:05:59):Succeed in initializing IS_OPERA.

(2017-11-14 15:38:01):No serial port available, check serial hardware.

(2017-11-14 15:38:04):Succeed in initializing IS_OPERA.

(2017-11-21 11:42:00):No serial port available, check serial hardware.

(2017-11-21 11:42:04):Succeed in initializing IS_OPERA.

(2017-11-21 11:58:51):No serial port available, check serial hardware.

(2017-11-21 11:58:55):Succeed in initializing IS_OPERA.

(2017-11-22 16:00:42):No serial port available, check serial hardware.

(2017-11-22 16:00:46):Succeed in initializing IS_OPERA.

(2017-11-22 16:02:42):No serial port available, check serial hardware.

(2017-11-22 16:02:44):Succeed in initializing IS_OPERA.

(2017-11-27 10:06:51):No serial port available, check serial hardware.

(2017-11-27 10:06:54):Succeed in initializing IS_OPERA.

(2017-11-28 19:13:23):No serial port available, check serial hardware.

(2017-11-28 19:13:28):Succeed in initializing IS_OPERA.

(2017-11-28 19:16:48):No serial port available, check serial hardware.

(2017-11-28 19:16:51):Succeed in initializing IS_OPERA.

(2017-11-29 22:07:41):No serial port available, check serial hardware.

(2017-11-29 22:07:43):Succeed in initializing IS_OPERA.

(2017-12-13 20:25:30):No serial port available, check serial hardware.

(2017-12-13 20:25:33):Succeed in initializing IS_OPERA.

(2017-12-23 11:03:26):No serial port available, check serial hardware.

(2017-12-23 11:03:32):Succeed in initializing IS_OPERA.

(2017-12-23 16:32:52):No serial port available, check serial hardware.

(2017-12-23 16:32:55):Succeed in initializing IS_OPERA.

(2017-12-26 11:12:56):No serial port available, check serial hardware.

(2017-12-26 11:12:58):Succeed in initializing IS_OPERA.

(2017-12-26 11:13:07):No serial port available, check serial hardware.

(2017-12-26 11:13:09):Succeed in initializing IS_OPERA.

(2017-12-27 17:30:50):No serial port available, check serial hardware.

(2017-12-27 17:30:53):Succeed in initializing IS_OPERA.

(2018-01-02 11:26:13):No serial port available, check serial hardware.

(2018-01-02 11:26:16):Succeed in initializing IS_OPERA.

(2018-01-03 12:39:29):No serial port available, check serial hardware.

(2018-01-03 12:39:32):Succeed in initializing IS_OPERA.

(2018-01-03 14:39:15):No serial port available, check serial hardware.

(2018-01-03 14:39:17):Succeed in initializing IS_OPERA.

(2018-01-03 17:24:40):No serial port available, check serial hardware.

(2018-01-03 17:24:42):Succeed in initializing IS_OPERA.

(2018-01-04 10:43:12):No serial port available, check serial hardware.

(2018-01-04 10:43:14):Succeed in initializing IS_OPERA.

(2018-01-04 15:23:23):No serial port available, check serial hardware.

(2018-01-04 15:23:26):Succeed in initializing IS_OPERA.

(2018-01-04 16:16:48):No serial port available, check serial hardware.

(2018-01-04 16:16:53):Succeed in initializing IS_OPERA.

(2018-01-04 16:17:42):[data exceeding range]:[function code H0014][range 100-9000][running value 0]

(2018-01-04 16:17:42):[data exceeding range]:[function code H0021][range 1-65535][running value 0]

(2018-01-04 16:20:41):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65534]

(2018-01-04 16:52:38):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-01-04 16:52:38):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2018-01-04 16:52:38):Succeed in initializing IS_OPERA.

(2018-01-04 16:55:39):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65535]

(2018-01-04 16:55:39):[data exceeding range]:[function code H0C14][range 1-4][running value 0]

(2018-01-04 16:56:23):[data exceeding range]:[function code H0011][range 1-65535][running value 0]

(2018-01-04 16:56:23):[data exceeding range]:[function code H0015][range 100-9000][running value 0]

(2018-01-04 16:56:23):[data exceeding range]:[function code H0017][range 2-360][running value 0]

(2018-01-04 16:56:23):[data exceeding range]:[function code H0021][range 1-65535][running value 0]

(2018-01-04 16:56:23):[data exceeding range]:[function code H0023][range 1-65535][running value 0]

(2018-01-04 16:59:57):Save a recipe file: E:\Projects\IS620P FC\20180104165941[IS620P_C].txt

(2018-01-04 17:03:11):Serial port 2 is not connected to the device.

(2018-01-04 17:03:11):Succeed in initializing IS_OPERA.

(2018-01-04 17:03:14):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-01-04 17:03:14):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2018-01-04 17:03:27):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-01-04 17:03:27):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2018-01-04 17:03:27):Succeed in initializing IS_OPERA.

(2018-01-09 12:47:01):Serial port 2 is not connected to the device.

(2018-01-09 12:47:01):Succeed in initializing IS_OPERA.

(2018-01-09 12:47:48):[data exceeding range]:[function code H0010][range 1-65535][running value 0]

(2018-01-09 12:47:48):[data exceeding range]:[function code H0012][range 10-65535][running value 0]

(2018-01-09 14:12:39):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65534]

(2018-01-09 14:12:39):[data exceeding range]:[function code H0C14][range 1-4][running value 0]

(2018-01-09 15:20:17):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-01-09 15:20:17):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2018-01-09 15:20:17):Succeed in initializing IS_OPERA.

(2018-01-09 16:47:47):No serial port available, check serial hardware.

(2018-01-09 16:47:54):Succeed in initializing IS_OPERA.

(2018-01-09 16:48:13):No serial port available, check serial hardware.

(2018-01-09 16:48:37):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-01-09 16:48:37):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-01-09 16:48:38):Succeed in initializing IS_OPERA.

(2018-01-09 18:15:31):Save a recipe file: E:\Projects\IS620P FC\20180109181518[IS620P_V] Shriram.txt

(2018-01-09 18:17:26):Save a recipe file: E:\Projects\IS620P FC\20180109181518[IS620P_V] Shriram.txt

(2018-01-29 14:36:42):Serial port 2 is not connected to the device.

(2018-01-29 14:36:43):Succeed in initializing IS_OPERA.

(2018-01-29 14:38:05):Save a recipe file: E:\Projects\Suyash Impex\X_Axis_20180129143741[IS620P_V].txt

(2018-01-29 14:38:41):8-N-2Fail to connect device.

(2018-01-29 14:38:47):8-N-2Fail to connect device.

(2018-01-29 14:39:01):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 2
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-01-29 14:39:01):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-01-29 14:39:02):Succeed in initializing IS_OPERA.

(2018-01-29 14:40:09):[data exceeding range]:[function code H0011][range 1-65535][running value 0]

(2018-01-29 14:40:09):[data exceeding range]:[function code H0013][range 10-65535][running value 0]

(2018-01-29 14:40:09):[data exceeding range]:[function code H0014][range 100-6000][running value 0]

(2018-01-29 14:40:09):[data exceeding range]:[function code H0017][range 2-360][running value 0]

(2018-01-29 14:41:24):Save a recipe file: E:\Projects\Suyash Impex\Z_Axis_20180129144115[IS620P_V].txt

(2018-01-29 14:41:36):Read a recipe file: E:\Projects\Suyash Impex\X_Axis_20180129143741[IS620P_V].txtInfo.:IS620P_V10.0_E.mdb


(2018-01-29 14:42:59):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-01-29 14:42:59):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-01-29 14:43:00):Succeed in initializing IS_OPERA.

(2018-01-29 14:43:42):[data exceeding range]:[function code H0022][range 1-65535][running value 0]

(2018-01-29 14:44:51):[data exceeding range]:[function code H0114][range 1-2000][running value 0]

(2018-01-29 14:45:26):Save a recipe file: E:\Projects\Suyash Impex\X_Axis_20180129143741[IS620P_V].txt

(2018-02-13 14:19:03):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-02-13 14:19:03):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-02-13 14:19:05):Succeed in initializing IS_OPERA.

(2018-02-13 15:00:16):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is  during parameter download.

(2018-02-13 15:00:16):Current software version of the servo:  00000320, database: IS620P_V10.0_E.mdb

(2018-02-16 11:34:17):No serial port available, check serial hardware.

(2018-02-16 11:34:20):Succeed in initializing IS_OPERA.

(2018-02-16 12:01:56):No serial port available, check serial hardware.

(2018-02-16 12:02:09):8-N-2Fail to connect device.

(2018-02-16 12:02:33):Serial port 2 is not connected to the device.

(2018-02-16 12:02:34):Succeed in initializing IS_OPERA.

(2018-02-16 12:02:51):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-02-16 12:02:51):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-02-20 12:14:05):Serial port 2 is not connected to the device.

(2018-02-20 12:14:06):Succeed in initializing IS_OPERA.

(2018-02-23 16:42:26):No serial port available, check serial hardware.

(2018-02-23 16:42:29):Succeed in initializing IS_OPERA.

(2018-02-24 10:25:30):No serial port available, check serial hardware.

(2018-02-24 10:25:32):Succeed in initializing IS_OPERA.

(2018-02-24 10:30:22):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-02-24 10:30:22):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-02-24 14:19:39):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-02-24 14:19:39):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-02-24 14:48:36):[data exceeding range]:[function code H0013][range 10-65535][running value 0]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0031][range 1-1073741824][running value 0]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0106][range 1-65535][running value 0]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0110][range 2000-20000][running value 300]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0113][range 2-128][running value 300]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0118][range 10-100][running value 300]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0127][range 1-65535][running value 0]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0130][range 500-1500][running value 0]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0144][range 0-3][running value 300]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0404][range 0-22][running value 300]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0521][range 1-65535][running value 0]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0903][range 0-3][running value 300]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0A15][range 1-1000][running value 0]

(2018-02-24 14:48:36):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65535]

(2018-02-24 14:48:36):[data exceeding range]:[function code H1752][range 0-1][running value 300]

(2018-02-24 15:17:34):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is  during parameter download.

(2018-02-24 15:17:34):Current software version of the servo:  00000064, database: IS620P_V10.0_E.mdb

(2018-02-24 15:17:36):Succeed in initializing IS_OPERA.

(2018-02-24 15:17:52):[data exceeding range]:[function code H1201][range 1-16][running value 0]

(2018-03-23 14:02:07):No serial port available, check serial hardware.

(2018-03-23 14:02:10):Succeed in initializing IS_OPERA.

(2018-05-10 11:32:33):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-05-10 11:32:33):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-05-10 11:32:34):Succeed in initializing IS_OPERA.

(2018-05-10 11:33:48):Save a recipe file: E:\Projects\Unique diamond\20180510113326[IS620P_V].txt

(2018-05-10 13:23:07):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-05-10 13:23:07):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-05-10 13:25:30):[data exceeding range]:[function code H0024][range 1-65535][running value 0]

(2018-05-10 13:25:30):[data exceeding range]:[function code H0107][range 1-65535][running value 0]

(2018-05-10 13:25:30):[data exceeding range]:[function code H0118][range 10-100][running value 0]

(2018-05-10 13:25:50):Save a recipe file: E:\Projects\Unique diamond\X-axis_20180510132538[IS620P_V].txt

(2018-05-10 13:26:31):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65534]

(2018-05-10 13:27:20):Save a recipe file: E:\Projects\Unique diamond\Y-axis_20180510132707[IS620P_V].txt

(2018-05-10 13:27:52):[data exceeding range]:[function code H0B01][range -9999-9999][running value 65535]

(2018-05-10 13:27:52):[data exceeding range]:[function code H0B02][range -3000-3000][running value 65478]

(2018-05-10 13:28:14):Save a recipe file: E:\Projects\Unique diamond\Z-axis_20180510132804[IS620P_V].txt

(2018-05-10 13:32:35):[data exceeding range]:[function code H0019][range 1-65535][running value 0]

(2018-05-10 13:32:35):[data exceeding range]:[function code H0105][range 1-65535][running value 0]

(2018-05-10 13:32:35):[data exceeding range]:[function code H0113][range 2-128][running value 0]

(2018-05-10 13:39:54):Save a recipe file: E:\Projects\Unique diamond\U-axis_20180510133944[IS620P_V].txt

(2018-05-10 13:40:40):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-05-10 13:40:40):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-05-10 13:40:41):Succeed in initializing IS_OPERA.

(2018-05-14 17:51:00):No serial port available, check serial hardware.

(2018-05-14 17:51:04):Succeed in initializing IS_OPERA.

(2018-05-21 13:02:36):No serial port available, check serial hardware.

(2018-05-21 13:02:39):Succeed in initializing IS_OPERA.

(2018-05-22 11:22:51):No serial port available, check serial hardware.

(2018-05-22 11:22:55):Succeed in initializing IS_OPERA.

(2018-05-22 12:54:36):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-05-22 12:54:36):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-05-22 12:54:37):Succeed in initializing IS_OPERA.

(2018-05-22 12:56:28):[data exceeding range]:[function code H0017][range 2-360][running value 0]

(2018-05-22 12:56:28):[data exceeding range]:[function code H0031][range 1-1073741824][running value 0]

(2018-05-22 12:56:28):[data exceeding range]:[function code H0105][range 1-65535][running value 0]

(2018-05-22 12:56:28):[data exceeding range]:[function code H0B21][range -1200-1200][running value 65535]

(2018-05-22 15:17:09):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-05-22 15:17:09):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-05-22 15:17:11):Succeed in initializing IS_OPERA.

(2018-06-06 18:35:04):No serial port available, check serial hardware.

(2018-06-06 18:35:07):Succeed in initializing IS_OPERA.

(2018-06-20 20:57:24):No serial port available, check serial hardware.

(2018-06-20 20:57:27):Succeed in initializing IS_OPERA.

(2018-07-01 22:10:14):No serial port available, check serial hardware.

(2018-07-01 22:10:17):Succeed in initializing IS_OPERA.

(2018-07-01 22:18:51):No serial port available, check serial hardware.

(2018-07-01 22:18:52):Succeed in initializing IS_OPERA.

(2018-07-01 22:19:04):No serial port available, check serial hardware.

(2018-07-01 22:19:06):Succeed in initializing IS_OPERA.

(2018-07-13 14:22:35):No serial port available, check serial hardware.

(2018-07-13 14:22:57):Succeed in initializing IS_OPERA.

(2018-07-13 14:24:32):Serial port 2 is not connected to the device.

(2018-07-13 14:24:44):8-N-2Fail to connect device.

(2018-07-13 14:24:55):8-E-1Fail to connect device.

(2018-07-13 14:27:47):Serial port 2 is not connected to the device.

(2018-07-13 14:27:47):Succeed in initializing IS_OPERA.

(2018-07-13 14:28:03):8-E-1Fail to connect device.

(2018-07-13 14:28:12):8-E-1Fail to connect device.

(2018-07-13 14:28:23):8-E-1Fail to connect device.

(2018-07-13 14:28:32):8-E-1Fail to connect device.

(2018-07-13 14:29:47):Serial port 2 is not connected to the device.

(2018-07-13 14:29:48):Succeed in initializing IS_OPERA.

(2018-07-13 14:30:04):8-E-1Fail to connect device.

(2018-07-13 14:30:46):8-N-2Fail to connect device.

(2018-07-13 15:05:04):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-07-13 15:05:04):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-07-13 15:05:05):Succeed in initializing IS_OPERA.

(2018-07-16 11:54:16):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-07-16 11:54:16):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-07-16 11:54:17):Succeed in initializing IS_OPERA.

(2018-07-16 11:58:45):[data exceeding range]:[function code H0D04][range 0-2][running value 3]

(2018-07-16 12:27:06):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-07-16 12:27:06):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2018-07-16 12:27:07):Succeed in initializing IS_OPERA.

(2018-07-16 12:27:20):Find a servo connection: 1. Serial port No.: COM2
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-07-16 12:27:20):Current software version of the servo:  00000001, database: IS620P_V10.0_E.mdb

(2018-07-16 12:27:21):Succeed in initializing IS_OPERA.

(2018-07-16 12:28:44):Set the local Database to : IS620P_V0006.4.mdb

(2018-07-16 12:28:44):Init Database Connection failed.

(2018-07-16 12:28:44):Get Data of Database Parameter failed.

(2018-07-16 12:28:44):Get Data of Database Groups failed.

(2018-07-16 12:28:44):Get Data of Database Customs failed.

(2018-07-16 12:55:13):[data exceeding range]:[function code H0B01][range -9999-9999][running value 64800]

(2018-07-16 12:55:13):[data exceeding range]:[function code H0B02][range -3000-3000][running value 65484]

(2018-07-16 12:55:25):[data exceeding range]:[function code H0B01][range -9999-9999][running value 64648]

(2018-09-14 14:06:54):Serial port 4 is not connected to the device.

(2018-09-14 14:06:55):Succeed in initializing IS_OPERA.

(2018-09-14 14:07:17):8-N-2Fail to connect device.

(2018-09-14 14:07:25):8-N-2Device connected successfully.

(2018-09-14 16:03:00):[data exceeding range]:[function code H0037][range 0-255][running value 65535]

(2018-09-14 16:04:23):Save a recipe file: C:\Users\TUSHAR\Desktop\Shahajanand\20180914160419[IS620P_C].txt

(2018-10-09 10:34:32):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-10-09 10:34:32):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2018-10-09 10:34:32):Succeed in initializing IS_OPERA.

(2018-10-09 10:37:11):[data exceeding range]:[function code H0013][range 10-65535][running value 0]

(2018-10-09 10:37:11):[data exceeding range]:[function code H0019][range 1-65535][running value 0]

(2018-10-09 10:37:11):[data exceeding range]:[function code H0021][range 1-65535][running value 0]

(2018-10-09 10:37:11):[data exceeding range]:[function code H0022][range 1-65535][running value 0]

(2018-10-09 10:37:11):[data exceeding range]:[function code H0024][range 1-65535][running value 0]

(2018-10-09 10:37:24):Save a recipe file: C:\Users\TUSHAR\Desktop\20181009103720[IS620P_C].txt

(2018-10-09 10:45:25):Find a servo connection: 1. Serial port No.: COM3
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-10-09 10:45:25):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2018-10-09 10:45:26):Succeed in initializing IS_OPERA.

(2018-10-09 10:46:05):[data exceeding range]:[function code H0010][range 1-65535][running value 0]

(2018-10-09 10:46:05):[data exceeding range]:[function code H0016][range 1-65535][running value 0]

(2018-10-09 10:46:05):[data exceeding range]:[function code H0021][range 1-65535][running value 0]

(2018-10-09 10:49:36):Save a recipe file: C:\Users\TUSHAR\Desktop\20181009104934[IS620P_C].txt

(2018-10-13 09:45:16):No serial port available, check serial hardware.

(2018-10-13 09:45:19):Succeed in initializing IS_OPERA.

(2018-10-13 10:15:35):No serial port available, check serial hardware.

(2018-10-13 10:15:37):Succeed in initializing IS_OPERA.

(2018-10-13 16:56:04):No serial port available, check serial hardware.

(2018-10-13 16:56:06):Succeed in initializing IS_OPERA.

(2018-10-13 16:58:29):No serial port available, check serial hardware.

(2018-10-13 16:58:30):Succeed in initializing IS_OPERA.

(2018-10-17 11:15:40):No serial port available, check serial hardware.

(2018-10-17 11:15:42):Succeed in initializing IS_OPERA.

(2018-10-17 11:33:43):8-N-2Device connected successfully.

(2018-10-17 13:18:40):8-N-2Fail to connect device.

(2018-10-19 09:34:10):No serial port available, check serial hardware.

(2018-10-19 09:34:18):Succeed in initializing IS_OPERA.

(2018-10-19 09:46:38):Serial port 5 is not connected to the device.

(2018-10-19 09:46:39):Succeed in initializing IS_OPERA.

(2018-10-19 10:09:31):Serial port 5 is not connected to the device.

(2018-10-19 10:09:31):Succeed in initializing IS_OPERA.

(2018-10-19 10:10:14):8-N-2Fail to connect device.

(2018-10-19 10:11:05):8-N-2Fail to connect device.

(2018-10-19 10:11:37):Set the local Database to : IS620P_CANopenV2.1_E.mdb

(2018-10-19 10:12:05):Succeed in initializing IS_OPERA.

(2018-10-19 10:12:06):Serial port 5 is not connected to the device.

(2018-10-19 10:12:22):8-N-2Fail to connect device.

(2018-10-19 10:13:16):8-N-2Device connected successfully.

(2018-10-19 10:13:49):Find a servo connection: 1. Serial port No.: COM5
2. Baud rate: :57600
3. Device ID: 1
 Note that 32-bit data transmission sequence of current Modbus is low 16 bits before high 16 bits during parameter download.

(2018-10-19 10:13:49):Current software version of the servo:  00000001, database: IS620P_CANopenV2.1_E.mdb

(2018-10-19 10:17:23):8-N-2Device connected successfully.

(2018-10-19 10:30:48):Completing search. No device is connected or serial port is used.

(2018-10-19 10:30:48):Succeed in initializing IS_OPERA.

(2018-10-19 10:35:30):Completing search. No device is connected or serial port is used.

(2018-10-19 10:35:31):Succeed in initializing IS_OPERA.

(2018-10-19 12:28:14):8-N-2Device connected successfully.

(2018-10-19 12:28:49):8-N-2Fail to connect device.

(2018-10-19 12:28:56):8-N-2Fail to connect device.

(2018-10-19 12:39:05):Succeed in initializing IS_OPERA.

(2018-10-19 12:39:05):Serial port 5 is not connected to the device.

(2018-10-19 12:39:14):Succeed in initializing IS_OPERA.

(2018-10-19 12:39:16):Serial port 5 is not connected to the device.

(2018-11-14 18:39:45):No serial port available, check serial hardware.

(2018-11-14 18:39:48):Succeed in initializing IS_OPERA.

(2018-11-14 18:48:48):No serial port available, check serial hardware.

(2018-11-14 18:48:51):Succeed in initializing IS_OPERA.

(2018-11-14 18:50:49):No serial port available, check serial hardware.

(2018-11-14 18:50:51):Succeed in initializing IS_OPERA.

(2018-11-14 18:51:23):No serial port available, check serial hardware.

(2018-11-14 18:51:26):Succeed in initializing IS_OPERA.

